B285 Molecule 4

GLASS LAMPSHADE

Ø 120 mm / Ø 4.7 "

GLASS

Borosilicate Transparent Glass

Borosilicate Transparent Glass (sandblasted inside)

WEIGHT

3,7 kg / 8,2 lb

LIGHT SOURCE

|  |  |
| --- | --- |
| LED Bulb (included) | 5 x 5 W |
| Max Wattage | 5 x 10 W |
| Total Lumens | 1800 – 2000 lm |
| Color Temperature | 2700 K |
| Bulb Base | E27 / E26 |
|  |  |

Dimmable with electronic dimmers only (ELV, trailing edge)